Herzlich Willkommen beim Damisoft Amiga Emulator
Diese Seite wurde von der Damisoft Groupe erstellt. Mit diesem Amiga Emulator kannst du fast alle Amiga Games in deinem Web Browser spielen.
Kurzanleitung:
In fünf kurzen Schritten bist du schon am Spielen.
1. Lade dir ein Spiel herunter und entpacke es gegeben Falls.
2. Lade dir ein Kickstart Rom herunter.
3. Klicke jetzt unten auf den Start Button und fuege links im Reiter ROM den heruntergeladenen Kickstart Rom ins oberste Feld ein.
4. Klicke anschliessend auf Floppy und füge bei DF0 die erste *.ADF Datei (Game) ein. DF0 ist das erste Diskettenlaufwerk. DF1 ist das zweite Diskettenlaufwerk usw....
5. Nun hast du alles vorbereitet was du brauchst. Zum Schluss klicke auf den Start Button um das Spiel zu starten.
Du kannst deine PC Tastatur zum Spielen benutzen. Leider hat jedes Spiel seine eigenen Tastaturkombinationen die du selber herausfinden musst.
Los gehts und viel Spass beim Spielen mit dem Amiga Emulator von Damisoft.
Um den Damisoft Amiga Emulator auszufuehren, klicke jetzt auf den Start Button.
Hinweis: Für dieses Projekt ist ein schneller Computer erforderlich.
Mobile- und Tablet-Geräte funktionieren moeglicherweise, haben aber hoechstwahrscheinlich eine zu langsame Bildrate.

Model ? | CPU | Chipset | Kickstart | Years
--- | --- | --- | --- | ---
|  | 68000 ? | OCS ? | 0.x-1.1 | 1985-87
|  | 68000 | OCS/ECS Agnus | 1.2-1.3 | 1987-91
| Amiga 2000 (default) | 68000 | ECS Agnus | 1.2-2.04 | 1987-92
|  | 68000 | ECS ? | 2.04 | 1991-92
|  | 68000 | ECS | 2.05 | 1992
|  | 68020 ? | AGA ? | 3.0-3.1 | 1992-96
| Amiga 3000 (no FPU and SCSI) | 68030 ? | ECS | 1.3-2.04 | 1990-92
| Amiga 4000/030 (no FPU) | 68030 | AGA | 3.0 | 1992-94
Model |  | Speed |
| 68000 (fake prefetching) |  | Original
| 68010 (fake prefetching) |  | Maximum
| 68020 |
| 68030 (fake MMU) |
Options |
| Compatible (enable prefetching and caches, slower but more compatible)
| 32bit address-space (required for Zorro3-memory or A3000/A4000 roms)
Type |  | Region |
| Original Chip Set (OCS) |  | PAL (50 Hz)
|  |  | NTSC (60 Hz)
| Advanced Graphics Architecture (AGA) |
Collisions |  | Blitter ? |
Mode |  |  | Immediate
|  | Waiting
Features |
Model |
Gayle | ? | RTC | ?
Onboard IDE |  | Type |
| PCMCIA slot (A600/A1200) |
CIA | ? | Misc |
TOD source |  |  | A1000 Agnus (8361/8367)
| TOD bug |  | Mirror ROM at $A80000
| Overlay ROM |  | Mirror ROM at $E00000
| A1000 Velvet-CIA (6526) |  | ZorroIII (A3000/A4000)
Onboard |  | RAMSEY | (A3000/A4000) ?
Chip |  | Onboard Fast | (Low)
Slow | (Bogo) | CPU-board Fast | (High)
ZorroII | ? | ZorroIII | (A3000/A4000) ?
Fast |  | Fast |
| AutoConfig™ ? | Mapping |
Kickstart |
Extended |
<unset>
Keyfile (Cloanto) |
<unset>
Macintosh (AMAX) |
<unset>
Image |  | File |
Type |  | Size |
Version |  | CRC-32 |
Encrytion |  | Checksum |
System |
Models |  | CPN |
CPUs |  |
Disk Floppies
DF0 |
|  | RO
<empty>
DF1 |
|  | RO
<empty>
DF2 |
|  | RO
<empty>
DF3 |
|  | RO
<empty>
Options
Speed | ('Turbo' mode is fastest, but not always compatible)
| Auto convert to ADF-EXT2
Note: Supported types are uncompressed ADF, DMS, IMG, EXE and SCP files. Insert an entry from the database:
Create a standard or custom (EXT2) disk-image: Label FFS Bootable
Disk |  | File |
Label |  | Size |
Type |  | CRC-32 |
Bootblock
Type |  | Checksum |
Data |
Onboard IDE (A600/A1200/A4000)
IDE0 |
|  | Media ATA RO
<empty>
IDE1 |
|  | Media ATA RO
<empty>
IDE2 |
|  | Media ATA RO
<empty>
IDE3 |
|  | Media ATA RO
<empty>
PCMCIA slot (A600/A1200)
SRAM |
|  | RO
<empty>
HD |
<empty>
Note: Supported types are uncompressed HDF and VHD files.
Drive |  | Partition |
Surfaces |  | Name |
Sectors |  | Reserved |
Blocksize |  | Bootpri |
Enabled
Driver |  | Cursor |
Mode |  | Mode |
| Antialias (WebGL only)
Resolution |  | Centering |
Horizontal |  |  | Horizontal
Vertical |  |  | Vertical
Interlace |
Colors |  | Alpha | (RGBA-modes only)
Brightness | (-1000 to 1000) | Background | (#rrggbb) ?
Contrast | (-1000 to 1000) | Blend | (0 to 255)
Gamma | (-1000 to 1000) |
| Blacker than black |
Misc |  | Debug |
| Frameskip |  | Refresh-indicator
Note: Driver is forced to 'Canvas' because 'WebGL' is not supported by this browser. Note: Video is disabled because 'Canvas'/'WebGL' is not supported by this browser. Enabled
Driver |
Buffer | frames (you may experiment with this value)
Basic |  | Lowpass filter |
Mode |  | Mode |
Frequency |  | Model |
Channels |
Stereo mixing |  | Interpolation |
Separation |  | Type |
Delay |
Note: Mode is forced to 'Off (emulated)' because 'WebAudio' is not supported by this browser.
Mouse |  | Move Fire 1 Fire 2 Device |
Game |  | Move Fire 1 Fire 2 Device |
| Note: If a joystick-device get not detected, try to press some buttons on it.
Keyboard |
| Enabled (emulated joysticks do always work)
Hardware dongle |
Type |

2026 - Damisoft Groupe © | Amiga Games | Kickstart Roms | Damisoft Groupe

PWR | HD |  |  |  |  |  |